|  |  |  |
| --- | --- | --- |
| **CN** | **DESCRIPCIÓN** | **PAÍS** |
| 8505 11 00 99 | Products containing neodymium, iron and boron, or an alloy of samarium and cobalt in shape of square or rectangle, intended to become permanent magnets after magnetisation. They are in dimension of: - a length of 14 mm to 45 mm (± 0,2 mm), - of width 8 mm do 25 mm (± 0,2 mm), - of thickness from 1,5 mm and not more than 4,5 mm (± 0,2 mm). | ESLOVENIA |
| 8505 19 10 9 | Permanent magnets of agglomerated ferrite, in shape of square, rectangle, rings, tubes, bushings or collars: - a length of 17 mm or more, but not over 110 mm (± 0,2 mm), - of width 15 mm or more, but not over 75 mm (± 0,2 mm), - of thickness 5 mm or more, but not over 13 mm (± 0,2 mm), meant to be installed on rotor of electromotor that is used in applications in ventilation and airconditioning systems | ESLOVENIA |
| 8536.49 | Relays: - The coil operating voltage is between 12-24 VDC - Contact current carrying capacity is between 5-15A - Contact voltage between 80-270 VAC - The outer dimensions are 19x15.2x15.5 mm and sugar cubes-shaped - For use in the production of control board of white goods. | TURQUÍA |
| 8507.60.00 | Lithium-Ion (Li-Ion) Battery, with: — a voltage of 150 V or more but not more than 300 V, — a length of 290 mm or more but not more than 490 mm, — a width of 670 mm or more but not more than 1120 mm, — a height of 140 mm or more but not more than 230 mm, for use in the manufacture of motor vehicles of Chapter 87. | TURQUÍA |
| 8507.50.00 | Nickel-Metal Hydride (NiMh) Battery, with: — a voltage of 150 V or more but not more than 300 V, — a length of 300 mm or more but not more than 500 mm, — a width of 675 mm or more but not more than 1125 mm, — a height of 140 mm or more but not more than 235 mm, for use in the manufacture of motor vehicles of Chapter 87 | TURQUÍA |
| 8501.52.90.90 / 8501.53.81.90 | AC traction motor of the Interior Permanent Magnet Synchronous Motor (IPMSM) type which develops: - Torque output between 200 Nm and 400 Nm - Power output between 50kW and 200kW - Max speed no more than 12500 rpm for use in the manufacture of electric vehicles | ESPAÑA |
| 8507.60.00 | Mobile Phone Battery - a thickness is not more than 5 mm, - a width is not more than 80 mm, - a length is not more than 155 mm, - a nominal capacity of 1,000 mAh or more but not more than 10,000 mAh, - an internal resistance max. 200 mAh, - - a charging and nominal voltage 3.5V and above - a weight is not more than 150 g, - intended use of Smartphone production For use in the manufacture of products falling within subheading 8517.12.00 | TURQUÍA |
| ex 8504 31 80 | Electrical transformer with: — a capacity of 240 Watts, — an operating temperature range of + 10 °C or more, but not more than + 125 °C, — five inductively coupled copper wire windings, — 11 connection pins at the bottom and — dimensions of not more than 31,3 mm x 37,8 m x 25,8 mm | AUSTRIA |
| ex 8536 41 90 | Power relay with: — electromechanical and electromagnetical switching function, — a load current of 3 amperes or more but not exceeding 16 amperes, — a coil voltage of 5 volts or more but not exceeding 24 volts, — a distance between the connector pins of the load circuit not more than 15,6 mm | AUSTRIA |
| 85030099 | Stator body of stacked electrical sheet having - an inner diameter of 18 mm or more, but not more than 35 mm, - an outer diameter of 35 mm or more, but not more than 65 mm and - a length or 20 mm or more, but not more than 65 mm [of a kind used in the production of brushless electrical motors] | AUSTRIA |
| 85030099 | Deep drawn steel motor housing having - an inner diameter of 35 mm or more, but not more than 65 mm, - an outer diameter of 35 mm or more, but not more than 70 mm and - a length or 35 mm or more, but not more than 150 mm [of a kind used in the production of brushless electrical motors] | AUSTRIA |
| 85030099 | Rotor body of stacked electrical sheet having - a diameter of 18 mm or more, but not more than 35 mm and - a length or 20 mm or more, but not more than 65 mm [of a kind used in the production of brushless electrical motors] | AUSTRIA |
| 8507 60 00 | Integrated battery system in a metal case with holders, consisting of: - a lithium-ion battery with voltage of 48V (+/- 5V) and capacity of 0,44 kWh (+/- 0,5 kWh), - Battery Management System, - a relay, - a low voltage converter (DC/DC), - at least one connector - for use in the manufacture of mild-hybrid motor vehicles (2) | ESLOVAQUIA |
| 8528 59 00 | Complex electronic device with LCD touch screen display powered by a voltage of 12 - 14,4 V, containing: - LCD control processor, - GPS module, - Bluetooth module, - USB port, - radio signal tuner, - whether or not DAB module, - whether or not functions for cooperation with E-CALL, - whether or not an integrated control panel, - whether or not connectors for use in the manufacture of goods of Chapter 87 (2) | ESLOVAQUIA |